PROJECT DEVELOPMENT PHASE SPRINT-4

|  |  |
| --- | --- |
| Date | 21 November 2022 |
| Team ID | PNT2022TMID15090 |
| Project Name | Hazardous Area Monitoring for Industrial Plant powered by IOT |

**Code:**

#include <DHT.h> WiFiClient wifiClient; String data3;

#define DHTTYPE DHT11 #define DHTPIN 4

#define MQTPIN 34

DHT dht(DHTPIN, DHTTYPE);

#define ORG "22h49t"

#define DEVICE\_TYPE "NodeMCU" #define DEVICE\_ID "NodeMCU"

#define TOKEN "12345678" #define speed 0.034 void callback(char\* topic, byte\* playload, unsigned int payloadLength); char server[] = ORG ".messaging.internetofthings.ibmcloud.com"; char publishTopic[]

= "iot-2/evt/Data/fmt/json"; char topic[] = "iot- 2/cmd/test/fmt/String"; char authMethod[] = "use-token-auth"; char token[] = TOKEN; char clientId[] = "d:" ORG ":" DEVICE\_TYPE ":" DEVICE\_ID; PubSubClient client(server, 1883, callback , wifiClient);

void publishData(); String command;

String data = ""; long duration; float dist;

void setup()

{

Serial.begin(115200); dht.begin(); wifiConnect(); mqttConnect();

}

void loop() { publishData(); delay(500); if (!client.loop()) { mqttConnect();

}

}

void wifiConnect() {

Serial.print("Connecting to "); Serial.print("Wifi"); WiFi.begin("JerroldWi-Fi","75779901"); while (WiFi.status() != WL\_CONNECTED) { delay(500); Serial.print(".");

}

Serial.print("WiFi connected, IP address: "); Serial.println(WiFi.localIP());

}

void mqttConnect() {

if (!client.connected()) {

Serial.print("Reconnecting MQTT client to "); Serial.println(server); while (!client.connect(clientId, authMethod, token)) { Serial.print("."); delay(500);

}

initManagedDevice(); Serial.println();

}

void initManagedDevice() { if (client.subscribe(topic)) { Serial.println("IBM subscribe to cmd OK");

} else {

Serial.println("subscribe to cmd FAILED");

}

}

void publishData()

{

int sensorValue = analogRead(MQTPIN); //MQT 135 connected to GPIO 34 (Analog ADC1\_CH6)

Serial.print("AirQua=");

Serial.print(sensorValue, DEC); Serial.println(" PPM"); float humid = dht.readHumidity(); float temp = dht.readTemperature(true); String payload = "{\"Humidity\":"; payload += humid; payload += "}"; if (client.publish(publishTopic, (char\*) payload.c\_str())) { Serial.println("Publish OK");

}

payload = "{\"Temperature\":"; payload += temp; payload += "}"; if

(client.publish(publishTopic, (char\*) payload.c\_str())) { Serial.println("Publish OK");

}

payload = "{\"AirQuality\":"; payload += String(sensorValue); payload += "}"; if (client.publish(publishTopic, (char\*) payload.c\_str())) { Serial.println("Publish OK");

}

void callback(char\* subscribeTopic, byte\* payload, unsigned int payloadLength) { Serial.print("callback invoked for topic:");

Serial.println(subscribeTopic); for (int i = 0; i < payloadLength; i++) { dist += (char)payload[i];

}

Serial.println("data:" + data3); if (data3 == "lighton") { Serial.println(data3);

}

data3 = "";

}